H4500 Measuring for Mounting Types
 
Surface:
Cassette Width: Take 3 measurements: top, center, bottom
To the widest add: 4 1/2” total (width of the track is 2").
 Track Height: Full opening height, round up to next foot
 
Between Jamb:
 Cassette Width: Take 3 measurements: top, center, bottom
From the smallest deduct: 3/8” on each side, so 3/4" in total.
That is so you have some adjustability in track placement.
 
Angle brackets: 2” x 1”, provide a surface to mount the tracks to. Order
them to span the full opening height, rounding up to nearest foot. Then cut
to size at site.
 
Track height: Cassette is 4.5” high, so order track to height of opening and you
have 4.5” of error margin.
 
Recessed:
Cassette width:
a) Measure top, middle and bottom
b) Take widest measurement, add 2 1/16” on each side, so total 4 1/8” added
          
Cassette box: If cassette is recessed in a box, it should minimum be 6” wide and
9 1/2” height for access, and slightly longer than the cassette/roller tube you are mounting in the pocket.
 
Recessed Track Size: 2" x 1.25"
Track recesses: Should be 2 1/16” deep and 1 ¼” + 1/16”  wide to accommodate
the recessed track
 
Track height: At least height of opening, possibly more depending on
placement of cassette if it is in a box above opening


